**MB10 Multi - Biometric**

**T&A and Access Control Terminal**

**Features**

• Fingerprint, face, RFID and password 4 type verification mode

• High-speed identification less than 1 second

• TCP/IP Port for Internet connection

• Access Port available to control one lock and exit button

• Optional 5V 1900mAH UPS, standby up to 3 hours

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Product | | | MB10 | |
| Main | Biometric  RF Optional | | Fingerprint and Face  125kHz EM / 13.56MHz MIFARE | |
| Capacity | | Max User(1:N)  Max Fingerprint (1:N)  Max Face (1:N)  Max Record | | |
| Interface | TCP/IP  USB  Relay | | 10M/100M  USB 2.0 (Host)  1 Relay | |
| Hardware | LCD  Sound  Operating Temp.  Operating Humidity  Power  Dimensions(W x H x D mm) | | 2.8” Color LCD  Stereo speaker  0 °C- 45 °C  20% ~ 80%  DC 5V 0.8A  167.9 x 151.5 x 30 | |
| Function | Standard | | Automatic Status Switch, Self-Service Query, DST, T9 Input  9 Digit User ID, Scheduled Bell, Photo ID  Lock, sensor, Exit button | |
| Optional | ID / MF | |
| Compatibility | | | ZKTime.net 3.0  ZKTime 5.0 | |